|  |  |
| --- | --- |
| ***H1 Cheat Sheet***  |  |
| **LOGIN** \*Power on your H1.\*Press the **OFFICER ID**, **PASSWORD**, **PARTNER ID** or **PATROL UNIT** fields for Virtual Keypad.\*Press **LOGIN** to advance to the home screen.  | **START/STOP RECORDING**\*Additionally, you can start recording using your trigger microphone. To stop recording using your trigger microphone, you can configure this button on the microphone. See your *COBAN H1 Adminstrator’s manual*. | \* Press **camera 1** to start recording with front camera\* Press **camera 2** to start recording with rear camera\* Press **camera 3** to start recording with extra camera\* Press the **camera** button again to stop recording.EDGE wireless mic copy.png |
| \*Once a recording is stopped, you will be prompted to enter data associated with the video. Enter the data, then click **Save**.  |
| **ICV/BWC VIDEO PLAYBACK** \*On the home screen, press the MENU  button to advance to the **FREQUENTLY USED** screen. |
|  | \* Press the **ICV VIDEO** or **BWC Video** buttons to play either In-car videos or Body Worn Camera videos.\* Select a video from the list, then press **PLAY**.  |  |
| **IN-CAR MIC** \*On the home screen, press the MENU  button to advance to the **FREQUENTLY USED** screen. |
|  | \*Press **IN-CAR MIC** to toggle the In-car Microphone on/off.  |
| **UPLOAD VIDEO** \*On the home screen, press the MENU  button to advance to the **FREQUENTLY USED** screen. |
|  | \*Tap **UPLOAD**.\*Press the buttons at the bottom to start/stop your ICV or BWC upload.  |  |

|  |
| --- |
| **FAILSAFE VIDEO PLAYBACK** \*On the home screen, tap the MENU  button to advance to the **FREQUENTLY USED** screen.While the camera is powered on, the system automatically records ALL activity and stores it to a failsafe drive. In the event of loss of data, the system will be able to retrieve damaged/removed data. |
|  | \* Press **FAILSAFE VIDEO.**\* Press a video, then press **PLAY**. | \*Review videos, bookmark or play at 2X speed |
| **TAKE SNAPSHOT/BOOKMARK** \*On the home screen, press the MENU  button to advance to the **Frequently Used** screen.  |
|  | \* Press the **SNAPSHOT** button. A confirmation message is displayed.    |
| **SWITCH OFFICER**  |
|  | \*Tap **SWITCH OFFICER**.\*Press in the designated boxes to input credentials with the virtual keypad, then tap **LOGIN**. |  |
| **SHUTDOWN**  |  |  |
|  | \* Press **SHUTDOWN**, then press **YES**.  |   |
| **MORE FUNCTIONS** |  |
|  | **LIVE** **AUDIO**: Press this button to playback live audio from microphone through the speakers. **VOLUME**: Press this button to adjust speaker volume. **LOG** **FILE**: Press this button to view the system log file. **SUMMARY**: Press this button to view details regarding the system’s platform, OS version, Firmware version, Software version, and the Build time for the software version **RUN** **STATUS**: Press this button to view the status of the current session. |